1. COMPACT LINE ARRAY SPEAKER

모델 : MYFIX, CPA10, CPA18S, CPA18SA

(1) 기  능

본 기기의 기능은 마이크를 통해서 들어온 전기적인 소리를 사람들이 들을 수 있는 음성 신호로 바꾸어 주는 일종의 에너지 변환장치인 듀얼 8인치의 라인어레이 스피커로 각종 음향 무대 공간에 설치가 가능하여야 하며, 다음의 성능 이상이어야 한다.

(2) 성  능

[Passive Speaker]

- System : 2-WAY FULL RANGE

- Rated Power : LF: 350W, HF: 100W

- Peak Power : LF: 1400W, HF: 400W

- Nominal Impedance : 16Ω

- Frequency Response : 80Hz – 18kHz

- Sensitivity : LF: 98dB, HF: 113dB

- Maximum SPL : LF: 123dB, HF: 133dB

- Coverage Angle : 100 × 10° (H×V)

- Woofer Unit : 1 × 10″

- Tweeter Unit : 1 × 3″

- Input Connection : 2 × NL4 LF: ±2 HF: ±1

- Dimensions (W×H×D) : 349 × 308× 332mm

- Net Weight : 15kg

[Passive Subwoofer Speaker]

- System : PASSIVE SUBWOOFER

- Rated Power : 800W

- Peak Power : 3200W

- Nominal Impedance : 8Ω

- Frequency Response : 34Hz – 250Hz

- Sensitivity : 97dB

- Maximum SPL : 126dB

- Coverage Angle : 360° (Omni)

- Woofer Unit : 1 × 18″

- Input Connection : 2 × NL4 LF: ±1

- Dimensions (W×H×D) : 530 × 660 × 700mm

- Net Weight : 50kg

[Active Subwoofer Speaker]

- System : ACTIVE SUBWOOFER

- Rated Power : 800W

- Peak Power : 3200W

- Amp Power : 1200W + 1200W + 1200W

- Nominal Impedance : 8Ω

- Frequency Response : 34Hz – 250Hz

- Sensitivity : 97dB

- Maximum SPL : 126dB

- Coverage Angle : 360° (Omni)

- Woofer Unit : 1 × 18″

- Input Connection : 2 × NL4 LF: ±1

- Operating Voltage : AC 220V 50/60Hz

- Dimensions (W×H×D)  : 530 × 660 × 700mm

- Net Weight  : 56kg

- 동등 또는 이상 품이어야 한다.