1. WIRELESS MIC RECEIVER

모델 : MYFIX, HW-910R

(1) 기  능

본 기기는 1채널 무선마이크용 수신기로써, 끊김 없는 다이버시티 수신 시스템이 적용되어 있으며, 각 채널에는 주파수 채널링을 완전히 제거하기 위해 독립적인 ID 코드가 제공되며, IR버튼으로 편리한 송수신 세팅이 가능하며, 송수신 거리 조절 기능이 탑재된 기기로 다음의 성능 이상이어야 한다.

(2) 성  능

[Receiver]

- Frequency range : 925.0 ~ 937.5MHz

- Frequency stability : 0.002PPM

- Receiving sensitivity : -100dB

- Tone frequency response : 60hz-18kHz (3dB)

- Harmonic distortion : < 0.5%

- Signal to noise ratio : ＞105dB

- Dynamic range : 105dB

- Maximum frequency offset : ±48KHz

- Stray suppression : ≥75dB

- Audio output : Balanced and unbalanced output

- Power supply : 12-18V DC/1000mA

- Dimensions (W x H x D) : 210x45x160mm

- Weight : 542g

[Transmitter]

- Frequency range: 925.5~937.25MHz

- Output power: 5mW / 15mW

- Spurious emission: < -70dBc

- Bandwidth: 60MHz

- Maximum modulation depth: ±48kHz

- Frequency response: 60~15kHz

- Signal to noise ratio: > 105dB

- Distortion: < 0.5%

- Input voltage range: mic 1V max

- Power supply: 2 × 1.5V (AA)

- Battery life: 10 hours

- Dimensions (W x H x D) : Hand: 275(L)x48(Ø)mm, Beltpack: 64x84x21mm

- Weight : Hand: 324g, Beltpack: 114g

- 동등 또는 이상 품이어야 한다.