1. ACTIVE LINE ARRAY SPEAKER

모델 : MYFIX, Mighty6

(1) 기  능

본 기기의 기능은 마이크를 통해서 들어온 전기적인 소리를 사람들이 들을 수 있는 음성 신호로 바꾸어 주는 일종의 에너지 변환장치인 앰프내장형 6개의 4.2인치 라인어레이 스피커로 DSP 내장 및 볼륨컨트롤이 가능한 기기로 각종 음향 무대 공간에 설치가 가능하여야 하며, 다음의 성능 이상이어야 한다.

(2) 성  능

- Type : 2 way active vented design

- Frequency Response : 65 ~ 20kHz

- Maximum SPL : 132dB

- Crossover Point : 630Hz

- Sensitivity input Selectable : +3dBV, 0dBV, -3dBV, -6dBV

- Driver LF : 6 x 4.2" woofer + 6 x 2" full range line array

- Dispersion Angle (H x V) : H 120˚ x V 10˚

- Signal Connectors (I/O) : Input : XLR | Output : XLR link

- Power I/O : POWERCON

- Volume : Volume control

- Amplifier : Class-D

- Power output (RMS) : LF: 500W + HF: 500W TOTAL 1000W

- Power output (MAX) : LF: 1000W + HF: 1000W TOTAL 2000W

- Feature functions : DSP Setup Switching power design LED power / signal
/ clip indicator FIR filter design, flat phase curve

- Cabinet : Birch Plywood with polyurea painted finish

- Grille : 1.0mm steel

- Pole support : Double holes 35mm Steel bottom holder

- Rigging and handling : Inter-enclosure angles 0,1,2,3,4,6,8,10˚

- Built-in Pin Lock support : 5 points

- Flybar support : Flybar+rope

- Fuse : T4AL 250V

- Operating voltage : AC 220V-240V, ~50/60Hz

- Dimensions (H x W x D) : 367 x 315 x 402mm

- Net Weight : 13.6kgs

- 동등 또는 이상 품이어야 한다.