1. ACTIVE LINE ARRAY SUBWOOFER SPEAKER

모델 : MYFIX, Mighty6 SUB

(1) 기  능

본 기기의 기능은 마이크를 통해서 들어온 전기적인 소리를 사람들이 들을 수 있는 음성 신호로 바꾸어 주는 일종의 에너지 변환장치인 15인치의 앰프내장형 서브우퍼 스피커로 각종 음향 무대 공간에 설치가 가능하여야 하며, 다음의 성능 이상이어야 한다.

(2) 성  능

- Type : Active vented subwoofer

- Frequency Response : 40 ~ 120Hz

- Maximum SPL : 134dB

- Crossover Point : Selectable 100Hz, 120Hz

- Driver LF : 15" subwoofer, 3" Voice Coil

- Signal Connectors (I/O) : Input  :  2 x XLR | Output  :  2 x XLR link

- Power I/O : POWERCON

- Volume : Volume control

- Amplifier : Class-D

- Power output (RMS) : 1000W

- Power output (MAX) : 2000W

- Feature functions : LCD with multiple DSP, Switching power design

LED power / signal / clip indicator, Phase switchable (0/180)

Delay value adjust, 100ms max

- Cabinet : Birch Plywood with polyurea painted finish

- Grille : 1.5mm steel

- Pole support : M20 screw pole

- Rigging and handling : Inter-enclosure angles 0˚ (Stacking)

- Flybar support : T6.35AL 250V

- Operating voltage : AC 220V-240V, ~50/60Hz

- Dimensions (H x W x D) : 623 x 443 x 660mm

- Net Weight : 37.5kgs

- 동등 또는 이상 품이어야 한다.