1. WIRELESS MIC SYSTEM

모델 : MYFIX, PW-920R, PW-900D

(1) 기  능

본 기기는 2채널 무선마이크 시스템으로써, 끊김 없는 다이버시티 수신 시스템이 적용되어 있으며, 각 채널에는 주파수 채널링을 완전히 제거하기 위해 독립적인 ID 코드가 제공되며, IR버튼으로 편리한 송수신 세팅이 가능하며, 송수신 거리 조절 기능이 탑재된 기기로 다음의 성능 이상이어야 한다.

(2) 성  능

<수신기>

- Carrier frequency band: 925.0 ~ 937.5MHz

- Oscillation mode: DPLL digital phase-locked loop technology

- Bandwidth: 50MHZ

- Frequency response: 50Hz～17KHz

- Receiving sensitivity: when the offset is equal to 35KHZ, When 6dBuV is input, S/N>58dB.

- Frequency stability: 0.005%

- Audio frequency offset: 75KHz@ distortion < 1%

- Comprehensive signal-to-noise ratio: S/N>95dB.

- Comprehensive T.H.D:<0.7%@1KHz

- Frequency response: 50Hz～17KHz

- Balanced output port: impedance 680 ohms,

- Unbalanced output audio port: impedance 2200 ohms

- Effective working distance: 100 meters (open place)

- Power supply: DC 12V-1000mA

- Size (WxDxH) : 482*44*180mm

<송신기>

- Carrier frequency band : 925.0 ~ 937.5MHz

- Modulation mode : Broadband FM

- Oscillation mode : DPLL digital phase-locked loop technology

- Harmonic radiation : More than 45dBm lower than the main wave

- Radio frequency power : Low power 5mW, high power 25mW

- Audio frequency offset : 75KHz@ distortion < 1%

- Frequency response : 50Hz～17KHz (±3dBm)

- Tone mode : Moving coil microphone

- Current consumption : 130mA

- Battery life : 10h

- Battery : AA*2(1.5V)

- Size (WxDxH)  : 257*50mm

- 동등 또는 이상 품이어야 한다.