1. WIRELESS WIRELESS TRANSMITTER

모델 : MYFIX, X-EAR

(1) 기  능

본 기기는 인이어 모니터 시스템의 트랜스미터로 원거리에도 안정된 RF 송신이 가능하며, IR 싱크 기능으로 간편한 세팅이 되며 감도 조절 기능이 탑재된 기기로 다음의 성능 이상이어야 한다.

(2) 성  능

[송신기]

- Carrier frequency range : 925MHz-937.5MHz

- Oscillation mode : PLL frequency synthesis

- RF out power : 13.5dBm

- Carrier error : 0.01%

- Harmonic radiation : -32dBm

- Modulation : FSK

- Nominal/maximum frequency deviation : ±65KHz

- Stereo input interface : phone Φ6.3mm *2, XLR composite socket*2

- Input impedance : 2.2KΩ

- Input gain range : 36 adjustable settings by every 1dB step

- Power supply : DC 12V/1A

- Working current : 350mA

- Dimensions : 210 * 44 * 150mm

- Net weight : 526 g

[수신기]

- Carrier frequency range : 925MHz-937.5MHz

- Receiving mode : Superheterodyne

- Image suppression : 45dBm

- RF sensitivity : when input is 10dBu, S/N ≥45dB

- SQ adjustment : built-in setting parameters

- Headphone output power : 80mW@16Ω

- Output level adjustment range : 30 levels adjustable, attenuation adjustment at every 1dB step

- Power requirement : AA1.5 batteries *2

- Working current : 3V 160mA

- Battery life : ≥6 hours

- Dimensions : 77.5 * 63 * 19.5mm

- Net weight(without battery) : 66.8g

- 동등 또는 이상 품이어야 한다.